[index] CentreCOM x510シリーズ・AT-IX5-28GPX コマンドリファレンス 5.4.3

# ipv6 ospf display route single-line

モード: グローバルコンフィグモード
カテゴリー: IPv6ルーティング / 経路制御（OSPFv3）

`(config)# ipv6 ospf display route single-line`

`(config)# no ipv6 ospf display route single-line`

show ipv6 ospf routeコマンドで表示される経路情報を1行で表示できるように表示形式を変更する

### 使用例

■ show ipv6 ospf routeコマンドで表示される経路情報を1行で表示できるように表示形式を変更する

    awplus# show ipv6 ospf route ↓
    OSPFv3 Process (*null*)
    Codes: C - connected, D - Discard, O - OSPF, IA - OSPF inter area
           E1 - OSPF external type 1, E2 - OSPF external type 2

       Destination                                   Metric
         Next-hop
    C  10:10::/64                                         1
         directly connected, vlan10, Area 0.0.0.0
    O  10:20::/64                                         2
         via fe80::20e:84ff:fe64:20c2, vlan30, Area 0.0.0.0
         via fe80::200:cdff:fe37:1, vlan10, Area 0.0.0.0
    C  10:30::/64                                         1
         directly connected, vlan30, Area 0.0.0.0
    E2 172:16:210::/64                                 1/20
         via fe80::200:cdff:fe37:1, vlan10
    E2 172:16:220::/64                                 1/20
         via fe80::200:cdff:fe37:1, vlan10
    IA 192:168:110::/64                                   2
         via fe80::200:cdff:fe37:1, vlan10, Area 0.0.0.0
    C  192:168:120::/64                                   1
         directly connected, vlan120, Area 0.0.0.1

    awplus# configure terminal ↓
    awplus(config)# ipv6 ospf display route single-line ↓
    awplus(config)# exit ↓
    awplus# show ipv6 ospf route ↓
    OSPFv3 Process (*null*)
    Codes: C - connected, D - Discard, O - OSPF, IA - OSPF inter area
           E1 - OSPF external type 1, E2 - OSPF external type 2

       Destination       Metric Next-hop
    C  10:10::/64        1      directly connected, vlan10, Area 0.0.0.0
    O  10:20::/64        2      via fe80::20e:84ff:fe64:20c2, vlan30, Area 0.0.0.0
                                via fe80::200:cdff:fe37:1, vlan10, Area 0.0.0.0
    C  10:30::/64        1      directly connected, vlan30, Area 0.0.0.0
    E2 172:16:210::/64   1/20   via fe80::200:cdff:fe37:1, vlan10
    E2 172:16:220::/64   1/20   via fe80::200:cdff:fe37:1, vlan10
    IA 192:168:110::/64  2      via fe80::200:cdff:fe37:1, vlan10, Area 0.0.0.0
    C  192:168:120::/64  1      directly connected, vlan120, Area 0.0.0.1

### コマンドツリー

`configure terminal (特権EXECモード)
|
+- ipv6 ospf display route single-line（グローバルコンフィグモード）
`

### 関連コマンド

show ipv6 ospf route（非特権EXECモード）

(C) 2012 - 2014 アライドテレシスホールディングス株式会社

PN: 613-001763 Rev.F