[index] CentreCOM x510シリーズ・AT-IX5-28GPX コマンドリファレンス 5.4.3

# terminal monitor

モード: 特権EXECモード
カテゴリー: 運用・管理 / ログ

`# terminal [no] monitor`

本コマンドを入力した端末において、ターミナルモニター（端末画面へのmonitorログの表示）を有効にする。各端末からログインした直後は無効。
「terminal no monitor」の形式で実行した場合はターミナルモニターを無効にする。
monitorログは初期状態で定義されているログ出力先の1つで、初期設定ではすべてのメッセージ（debuggingレベル以上のメッセージ）が出力されるようになっている。出力されるメッセージの条件は、log(filter)コマンドで変更できる。
なお、ターミナルモニターは現行のログインセッションにおいてのみ有効なので、ログアウトすると無効になる。

### 使用例

    awplus# terminal monitor ↓
    awplus#06:30:14 syslog-ng[799]: SIGHUP received, reloading configuration;
    06:30:59 HSL[1191]: HSL: nbytes -1
    06:30:59 HSL[1191]: HSL: INFO: Adding nexthop c0a80aea (000c.2928.1893) on interface vlan10
    06:31:01 crond[877]: USER manager pid 12242 cmd rotate_logs
    06:31:14 syslog-ng[799]: Log statistics; dropped=\'pipe(/dev/ttyS0)=0\', dropped
    =\'program(/usr/bin/corerotate)=0\', processed=\'center(queued)=4\', processed=\
    'center(received)=4\', processed=\'destination(d_buffered)=0\', processed=\'dest
    ination(d_ttyS0)=4\', processed=\'destination(d_stats)=0\', processed=\'destinat
    ion(d_permanent)=0\', processed=\'destination(d_exception_log)=0\', processed=\'
    destination(d_corefile)=0\', processed=\'source(s_src)=4\'
    06:31:35 dhcpd: ip length 328 disagrees with bytes received 332.
    06:31:35 dhcpd: accepting packet with data after udp payload.
    06:31:35 dhcpd: DHCPRELEASE of 192.168.10.234 from 00:0c:29:28:18:93 via vlan10 (found)
    06:31:46 dhcpd: ip length 328 disagrees with bytes received 332.
    06:31:46 dhcpd: accepting packet with data after udp payload.
    06:31:46 dhcpd: DHCPDISCOVER from 00:0c:29:28:18:93 via vlan10
    06:31:47 dhcpd: DHCPOFFER on 192.168.10.234 to 00:0c:29:28:18:93 via vlan10
    06:31:47 dhcpd: ip length 328 disagrees with bytes received 332.
    06:31:47 dhcpd: accepting packet with data after udp payload.
    06:31:47 dhcpd: DHCPREQUEST for 192.168.10.234 (192.168.10.1) from 00:0c:29:28:18:93 via vlan10
    06:31:47 dhcpd: DHCPACK on 192.168.10.234 to 00:0c:29:28:18:93 via vlan10
    06:31:47 HSL[1191]: HSL: INFO: Adding nexthop c0a80aea (000c.2928.1893) on interface vlan10

### 注意・補足事項

■ コンソールターミナルから本コマンドを実行したとき、「% Warning: Console logging may be enabled」というメッセージが表示される。これは、consoleログが有効化されている場合（初期設定で有効。ただし、出力条件はcriticalレベル以上）、consoleログとmonitorログに同じメッセージが出力され、表示が重複する可能性があることを示している。
■ 本コマンドは、複数ノードを対象とするワーキングセットプロンプト（atmf working-set）では実行できない（下記メッセージが出てエラーになる）。1台のノードだけを対象とするワーキングセットプロンプトか、ローカルプロンプトから実行すること。

    % Working set must contain only single node for this command

### 関連コマンド

log（グローバルコンフィグモード）
log(filter)（グローバルコンフィグモード）
show log config（非特権EXECモード）

(C) 2012 - 2014 アライドテレシスホールディングス株式会社

PN: 613-001763 Rev.F