[index] CentreCOM x510シリーズ・AT-IX5-28GPX コマンドリファレンス 5.4.3

# show ipv6 ospf interface

モード: 非特権EXECモード
カテゴリー: IPv6ルーティング / 経路制御（OSPFv3）

`> show ipv6 ospf interface [IFNAME]`

OSPFv3インターフェースの情報を表示する。

### パラメーター

`IFNAME` | インターフェース名。省略時はすべてのOSPFv3インターフェースが対象となる

### 使用例

    awplus> show ipv6 ospf interface ↓
    vlan10 is up, line protocol is up
      Interface ID 210
      IPv6 Prefixes
        fe80::21a:ebff:fe33:c549/64 (Link-Local Address)
        10:10::2/64

      OSPFv3 Process (*null*), Area 0.0.0.0, Instance ID 0
        Router ID 2.2.2.2, Network Type BROADCAST, Cost: 1
        Transmit Delay is 1 sec, State DR, Priority 1
        Designated Router (ID) 2.2.2.2
          Interface Address fe80::21a:ebff:fe33:c549
        Backup Designated Router (ID) 1.1.1.1
          Interface Address fe80::200:cdff:fe37:1
        Timer interval configured, Hello 10, Dead 40, Wait 40, Retransmit 5
          Hello due in 00:00:02
        Neighbor Count is 1, Adjacent neighbor count is 1
    vlan30 is up, line protocol is up
      Interface ID 230
      IPv6 Prefixes
        fe80::21a:ebff:fe33:c549/64 (Link-Local Address)
        10:30::2/64

      OSPFv3 Process (*null*), Area 0.0.0.0, Instance ID 0
        Router ID 2.2.2.2, Network Type BROADCAST, Cost: 1
        Transmit Delay is 1 sec, State DR, Priority 1
        Designated Router (ID) 2.2.2.2
          Interface Address fe80::21a:ebff:fe33:c549
        Backup Designated Router (ID) 3.3.3.3
          Interface Address fe80::20e:84ff:fe64:20c2
        Timer interval configured, Hello 10, Dead 40, Wait 40, Retransmit 5
          Hello due in 00:00:01
        Neighbor Count is 1, Adjacent neighbor count is 1
    vlan120 is up, line protocol is up
      Interface ID 320
      IPv6 Prefixes
        fe80::21a:ebff:fe33:c549/64 (Link-Local Address)
        192:168:120::2/64

      OSPFv3 Process (*null*), Area 0.0.0.1, Instance ID 0
        Router ID 2.2.2.2, Network Type BROADCAST, Cost: 1
        Transmit Delay is 1 sec, State DR, Priority 1
        Designated Router (ID) 2.2.2.2
          Interface Address fe80::21a:ebff:fe33:c549
        No backup designated router on this link
        Timer interval configured, Hello 10, Dead 40, Wait 40, Retransmit 5
          Hello due in 00:00:03
        Neighbor Count is 0, Adjacent neighbor count is 0

(C) 2012 - 2014 アライドテレシスホールディングス株式会社

PN: 613-001763 Rev.F