[index] CentreCOM x510シリーズ・AT-IX5-28GPX コマンドリファレンス 5.4.3

# show ipv6 ospf database router

モード: 非特権EXECモード
カテゴリー: IPv6ルーティング / 経路制御（OSPFv3）

`> show ipv6 ospf database router [A.B.C.D] [adv-router A.B.C.D|self-originate]`

リンク状態データベース（LSDB）に格納されているルーターLSA（タイプ1LSA）の内容を表示する。

### パラメーター

`A.B.C.D` | リンク状態ID（Link State ID欄）が指定値と一致するLSAだけを表示する
`adv-router A.B.C.D` | 広告元ルーター（Advertising Router欄）が指定値と一致するLSAだけを表示する
`self-originate` | 広告元ルーター（Advertising Router欄）が自身のルーターIDと一致するLSAだけを表示する

### 使用例

    awplus> show ipv6 ospf database router ↓

                OSPFv3 Router with ID (2.2.2.2) (Process *null*)

                    Router-LSA (Area 0.0.0.0)

      LS age: 1563
      LS Type: Router-LSA
      Link State ID: 0.0.0.0
      Advertising Router: 1.1.1.1
      LS Seq Number: 0x80000088
      Checksum: 0x729F
      Length: 56
      Flags: 0x03 (-|-|E|B)
      Options: 0x000013 (-|R|-|-|E|V6)

        Link connected to: a Transit Network
          Metric: 1
          Interface ID: 220
          Neighbor Interface ID: 220
          Neighbor Router ID: 1.1.1.1

        Link connected to: a Transit Network
          Metric: 1
          Interface ID: 210
          Neighbor Interface ID: 210
          Neighbor Router ID: 2.2.2.2

      LS age: 1177
      LS Type: Router-LSA
      Link State ID: 0.0.0.0
      Advertising Router: 2.2.2.2
      LS Seq Number: 0x800000D5
      Checksum: 0x4D5B
      Length: 56
      Flags: 0x03 (-|-|E|B)
      Options: 0x000013 (-|R|-|-|E|V6)

        Link connected to: a Transit Network
          Metric: 1
          Interface ID: 230
          Neighbor Interface ID: 230
          Neighbor Router ID: 2.2.2.2

        Link connected to: a Transit Network
          Metric: 1
          Interface ID: 210
          Neighbor Interface ID: 210
          Neighbor Router ID: 2.2.2.2

      LS age: 1818
      LS Type: Router-LSA
      Link State ID: 0.0.0.0
      Advertising Router: 3.3.3.3
      LS Seq Number: 0x80000031
      Checksum: 0x680B
      Length: 56
      Flags: 0x02 (-|-|E|-)
      Options: 0x000033 (DC|R|-|-|E|V6)

        Link connected to: a Transit Network
          Metric: 1
          Interface ID: 2098
          Neighbor Interface ID: 230
          Neighbor Router ID: 2.2.2.2

        Link connected to: a Transit Network
          Metric: 1
          Interface ID: 2088
          Neighbor Interface ID: 220
          Neighbor Router ID: 1.1.1.1

                    Router-LSA (Area 0.0.0.1)

      LS age: 1464
      LS Type: Router-LSA
      Link State ID: 0.0.0.0
      Advertising Router: 2.2.2.2
      LS Seq Number: 0x80000034
      Checksum: 0x8275
      Length: 24
      Flags: 0x01 (-|-|-|B)
      Options: 0x000011 (-|R|-|-|-|V6)

### 関連コマンド

show ipv6 ospf database（非特権EXECモード）
show ipv6 ospf database external（非特権EXECモード）
show ipv6 ospf database network（非特権EXECモード）

(C) 2012 - 2014 アライドテレシスホールディングス株式会社

PN: 613-001763 Rev.F