[index] AT-AR3050S/AT-AR4050S/AT-AR4050S-5G コマンドリファレンス 5.5.4

# show l2tp session

モード: 特権EXECモード
カテゴリー: VPN / L2TPv2

`# show l2tp session [detail]`

L2TPv2セッションの情報を表示する。

### パラメーター

`detail` | 詳細な情報を表示したいときに指定する

### 使用例

    awplus# show l2tp session  ↓

    L2TP Session Information

    --------------------------------------------------------------------------------
    Session ID:                     59400
    Tunnel ID:                      25351
    State:                          RETRY
    Created At:                     May 31 20:03:04 2016
    Interface Name:                 ppp1
    Remote Session ID:              61156
    Establish Timeout:              120

    awplus# show l2tp session detail  ↓

    L2TP Session Information details

    Session 59400 on tunnel 25351:-
      type: LAC Incoming Call, state: ESTABLISHED
      created at:  May 31 20:03:04 2016
      administrative name: session_tunnel1
      interface name: ppp1
      created by admin: YES, peer session id: 41165
      session profile name: session_profile_tunnel1
      ppp profile name: ppp_profile_ppp1
      use data sequence numbers: OFF
      establish timeout: 120
      trace flags: PROTOCOL FSM API AVP FUNC XPRT DATA PPP SYSTEM
      framing types: SYNC ASYNC
      bearer types: DIGITAL ANALOG
      call serial number: 1
      sub address: 'office1'
    Status:-
      data rx packets: 4, rx bytes: 100, rx errors: 0
      data tx packets: 4, tx bytes: 132, tx errors: 0
      Peer configuration data:-
        framing types: NONE
        bearer types: NONE
      memory usage: 2011 bytes
      Events:-
        20:03:04 INCALL_IND in state IDLE, new state WAITTUNNEL
        20:03:04 TUNNEL_OPEN_IND in state WAITTUNNEL, new state WAITREPLY
        20:03:04 ICRP_ACCEPT in state WAITREPLY, new state ESTABLISHED
        20:03:40 CLOSE_REQ in state ESTABLISHED, new state IDLE
        20:04:41 TUNNEL_OPEN_IND in state IDLE, new state WAITREPLY
        20:04:41 ICRP_ACCEPT in state WAITREPLY, new state ESTABLISHED

### 関連コマンド

l2tp tunnel（グローバルコンフィグモード）
show l2tp tunnel（特権EXECモード）

(C) 2015 - 2024 アライドテレシスホールディングス株式会社

PN: 613-002107 Rev.BC