[index] CentreCOM AR550S コマンドリファレンス 2.9

# ADD SNMP TARGETPARAMS

カテゴリー：運用・管理 / SNMP

`ADD SNMP TARGETPARAMS=params SECURITYLEVEL={noAuthNoPriv|authNoPriv|authPriv} USER=username`

params: SNMPターゲットパラメーターセット名（1〜32文字。大文字小文字を区別する）
username: SNMPユーザー名（1〜32文字。大文字小文字を区別する）

（SNMPv3）ターゲット（通知メッセージの送信先）との通信に使用するパラメーターセット（セキュリティーレベルとユーザー名）を定義する。

パラメーター

TARGETPARAMS: SNMPターゲットパラメーターセット名

SECURITYLEVEL: 本ターゲットパラメーターセットにおいて求められるセキュリティーレベルを指定する。noAuthNoPriv（認証なし・暗号化なし）、authNoPriv（認証あり・暗号化なし）、authPriv（認証あり・暗号化あり）から選択する。USERパラメーターで指定したユーザーのセキュリティーレベルと同じレベルを指定すること。

USER: SNMPユーザー名。ADD SNMP USERコマンドで定義したユーザー名を指定する。

例

``■ SNMPターゲットパラメーターセット「pzein」を定義する。セキュリティーレベルはauthNoPriv（認証あり・暗号化なし）、ユーザー名はzeinとする。
`ADD SNMP TARGETPARAMS=pzein SECURITYLEVEL=authNoPriv USER=zein`

関連コマンド

ADD SNMP GROUP
ADD SNMP TARGETADDR
ADD SNMP USER
ADD SNMP VIEW
DELETE SNMP TARGETPARAMS
SHOW SNMP
SHOW SNMP GROUP
SHOW SNMP TARGETADDR
SHOW SNMP TARGETPARAMS
SHOW SNMP USER
SHOW SNMP VIEW

参考

RFC1155, Structure and Identification of Management Information for TCP/IP-based Internets
RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1239, Reassignment of Experimental MIBs to Standard MIBs
RFC1398, Definitions of Managed Objects for the Ethernet-like Interface Types
RFC1493, Definitions of Managed Objects for Bridges
RFC1514, Host Resources MIB
RFC1573, Evolution of the Interfaces Group of MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC2233, The Interfaces Group MIB using SMIv2
RFC2576, Coexistence between Version 1, Version 2, and Version 3 of the Internet-standard Network Management Framework
RFC2578, Structure of Management Information Version 2 (SMIv2)
RFC2579, Textual Conventions for SMIv2
RFC2580, Conformance Statements for SMIv2
RFC3410, Introduction and Applicability Statements for Internet Standard Management Framework
RFC3411, An Architecture for Describing Simple Network Management Protocol (SNMP) Management Frameworks
RFC3412, Message Processing and Dispatching for the Simple Network Management Protocol (SNMP)
RFC3413, Simple Network Management Protocol (SNMP) Applications
RFC3414, User-based Security Model (USM) for version 3 of the Simple Network Management Protocol (SNMPv3)
RFC3415, View-based Access Control Model (VACM) for the Simple Network Management Protocol (SNMP)
RFC3416, Version 2 of the Protocol Operations for the Simple Network Management Protocol (SNMP)
RFC3417, Transport Mappings for the Simple Network Management Protocol (SNMP)
RFC3418, Management Information Base (MIB) for the Simple Network Management Protocol (SNMP)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H