[index] CentreCOM AR550S コマンドリファレンス 2.9

# DESTROY BGP DAMPING PARAMETERSET

カテゴリー：IP / 経路制御（BGP-4）

`DESTROY BGP DAMPING PARAMETERSET={ALL|1..100}`

BGP-4ルートフラップダンピング用のパラメーターセットを削除する。
有効化されているパラメーターセットは削除できない。また、デフォルトのパラメーターセット（内部的な番号は0）も削除できない。

パラメーター

PARAMETERSET: パラメーターセット番号。ALLを指定した場合は、すべてのパラメーターセットが対象となる。

関連コマンド

ADD BGP PEER
CREATE BGP DAMPING PARAMETERSET
DISABLE BGP DAMPING
ENABLE BGP DAMPING
PURGE BGP DAMPING
RESET BGP DAMPING
SET BGP DAMPING PARAMETERSET
SHOW BGP DAMPING
SHOW BGP DAMPING ROUTES

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H