## CentreCOM AR550S 設定例集 2.9
##  111 PPPoEインターネット接続環境における2点間IPsec VPN（片側アドレス不定）
##  ルーターBのコンフィグ
##
## 「#」で始まる行は、コンソールから入力しないと意味を持たないコマンドです。

ADD USER=secoff PASSWORD=PasswordS PRIVILEGE=SECURITYOFFICER
CREATE PPP=0 OVER=eth0-ANY
SET PPP=0 OVER=eth0-ANY IPREQUEST=ON USER=user@ispB PASSWORD=isppasswdB LQR=OFF BAP=OFF ECHO=ON
ENABLE IP
ENABLE IP REMOTEASSIGN
ADD IP INT=vlan1 IP=192.168.20.1 MASK=255.255.255.0
ADD IP INT=ppp0 IP=0.0.0.0
ADD IP ROUTE=0.0.0.0 INT=ppp0 NEXTHOP=0.0.0.0
ENABLE FIREWALL
CREATE FIREWALL POLICY=net
ENABLE FIREWALL POLICY=net ICMP_F=PING,UNREACH
DISABLE FIREWALL POLICY=net IDENTPROXY
ADD FIREWALL POLICY=net INT=vlan1 TYPE=PRIVATE
ADD FIREWALL POLICY=net INT=ppp0 TYPE=PUBLIC
ADD FIREWALL POLICY=net NAT=ENHANCED INT=vlan1 GBLINT=ppp0
ADD FIREWALL POLICY=net RULE=1 AC=NONAT INT=vlan1 PROT=ALL IP=192.168.20.1-192.168.20.254
SET FIREWALL POLICY=net RULE=1 REMOTEIP=192.168.10.1-192.168.10.254
ADD FIREWALL POLICY=net RULE=2 AC=NONAT INT=ppp0 PROT=ALL IP=192.168.20.1-192.168.20.254 ENCAP=IPSEC
# CREATE ENCO KEY=1 TYPE=GENERAL VALUE="secret"
CREATE ISAKMP POLICY="i" PEER=4.4.4.1 KEY=1 HEARTBEATMODE=BOTH SENDN=TRUE LOCALID="client" MODE=AGGRESSIVE
CREATE IPSEC SASPEC=1 KEYMAN=ISAKMP PROTOCOL=ESP ENCALG=DES HASHALG=SHA
CREATE IPSEC BUNDLE=1 KEYMAN=ISAKMP STRING="1"
CREATE IPSEC POLICY="isa" INT=ppp0 ACTION=PERMIT LPORT=500 RPORT=500 TRANSPORT=UDP
CREATE IPSEC POLICY="vpn" INT=ppp0 ACTION=IPSEC KEYMAN=ISAKMP BUNDLE=1 PEER=4.4.4.1
SET IPSEC POLICY="vpn" LAD=192.168.20.0 LMA=255.255.255.0 RAD=192.168.10.0 RMA=255.255.255.0
CREATE IPSEC POLICY="inet" INT=ppp0 ACTION=PERMIT
ENABLE IPSEC
ENABLE ISAKMP
# LOGIN secoff
# ENABLE SYSTEM SECURITY_MODE
