[index] CentreCOM AR550S コマンドリファレンス 2.9

# ADD PPP ACSERVICE

カテゴリー：PPP / PPPoE AC

`ADD PPP ACSERVICE=service-name TEMPLATE=template ACINTERFACE=interface`

service-name: PPPoEサービス名（最大64文字）
template: PPPテンプレート番号（0〜31）
interface: IPインターフェース名（eth0、ppp0など）

PPPoEサービスを作成する。
これは、本ルーターをPPPoEサーバー（Access Concentrator）として利用するためのもの。

パラメーター

ACSERVICE: サービス名。クライアント側でこの名前を指定して接続する。

TEMPLATE: PPPテンプレート番号。クライアントが接続してきたときに動的に作成するPPPインターフェースのパラメーターをあらかじめ設定したもの。CREATE PPP TEMPLATEコマンドで作成する。

ACINTERFACE: AC（Access Concentrator）として動作するインターフェースを指定。

例

``■ PPPoEサービスの設定例
`ADD USER=usera PASSWORD=passworda LOGIN=NO
CREATE PPP TEMPLATE=1 BAP=OFF LQR=OFF AUTH=CHAP IPPOOL=addr
ENABLE PPP ACCESSCONCENTRATOR
ADD PPP ACSERVICE=joge TEMPLATE=1 ACINTERFACE=vlan1
ENABLE IP
CREATE IP POOL=addr IP=172.16.28.211-172.16.28.220
` ■ PPPoEクライアント側の設定例
`CREATE PPP=0 OVER=eth0-joge IPREQUEST=ON
SET PPP=0 USERNAME=usera PASSWORD=passworda
ENABLE IP
ENABLE IP REMOTEASSIGN
ADD IP INT=ppp0 IP=0.0.0.0
ADD IP ROUTE=0.0.0.0 MASK=0.0.0.0 INT=ppp0 NEXT=0.0.0.0`

関連コマンド

CREATE PPP TEMPLATE
DELETE PPP ACSERVICE
DISABLE PPP ACCESSCONCENTRATOR
ENABLE PPP ACCESSCONCENTRATOR
SET PPP ACSERVICE
SHOW PPP PPPOE
SHOW PPP TEMPLATE

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1378, The PPP AppleTalk Control Protocol (ATCP)
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1552, The PPP Internetwork Packet Exchange Control Protocol (IPXCP)
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC1962, The PPP Compression Control Protocol (CCP)
RFC1968, The PPP Encryption Control Protocol (ECP)
RFC1974, PPP Stac LZS Compression Protocol
RFC1978, PPP Predictor Compression Protocol
RFC1990, The PPP Multilink Protocol (MP)
RFC2125, The PPP Bandwidth Allocation Protocol (BAP) / The PPP Bandwidth Allocation Control Protocol (BACP)
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H