[index] CentreCOM AR550S コマンドリファレンス 2.9

# DISABLE PPP ACCESSCONCENTRATOR

カテゴリー：PPP / PPPoE AC

`DISABLE PPP ACCESSCONCENTRATOR`

PPPoEサーバー（Access Concentrator）機能を無効にする。デフォルトは無効

関連コマンド

CREATE PPP TEMPLATE
DESTROY PPP TEMPLATE
ENABLE PPP ACCESSCONCENTRATOR
SET PPP ACSERVICE
SHOW PPP
SHOW PPP PPPOE
SHOW PPP TEMPLATE

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1378, The PPP AppleTalk Control Protocol (ATCP)
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1552, The PPP Internetwork Packet Exchange Control Protocol (IPXCP)
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC1962, The PPP Compression Control Protocol (CCP)
RFC1968, The PPP Encryption Control Protocol (ECP)
RFC1974, PPP Stac LZS Compression Protocol
RFC1978, PPP Predictor Compression Protocol
RFC1990, The PPP Multilink Protocol (MP)
RFC2125, The PPP Bandwidth Allocation Protocol (BAP) / The PPP Bandwidth Allocation Control Protocol (BACP)
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H