[index] CentreCOM AR550S コマンドリファレンス 2.9

# DELETE SNMP COMMUNITY

カテゴリー：運用・管理 / SNMP

`DELETE SNMP COMMUNITY=community [MANAGER=ipadd[/masklen]] [TRAPHOST=ipadd] [V1TRAPHOST=ipadd] [V2CTRAPHOST=ipadd]`

community: SNMPコミュニティー名（1〜15文字。大文字小文字を区別する）
ipadd: IPアドレス
masklen: マスク長（0〜32）

（SNMPv1/v2c）SNMPコミュニティーから管理ステーション、トラップホストを削除する。

パラメーター

COMMUNITY: SNMPコミュニティー名

MANAGER: SNMPオペレーションを許可する管理ステーションを指定する。マスク長を付加することで範囲指定も可能。本製品は、MANAGERに登録されていないホストからのSNMP要求には応答しない。ただし、SNMPコミュニティーのOPENパラメーターがYESの場合は、MANAGERパラメーターの設定にかかわらず、すべてのSNMP要求に応答する。

TRAPHOST: SNMPv1トラップの送信先ホスト

V1TRAPHOST: SNMPv1トラップの送信先ホスト。TRAPHOSTパラメーターと同じ。

V2CTRAPHOST: SNMPv2cトラップの送信先ホスト

関連コマンド

ADD SNMP COMMUNITY
CREATE SNMP COMMUNITY
DESTROY SNMP COMMUNITY
DISABLE SNMP COMMUNITY
ENABLE SNMP COMMUNITY
SET SNMP COMMUNITY
SHOW SNMP COMMUNITY

参考

RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H