[index] CentreCOM AR550S コマンドリファレンス 2.9

# SHOW PPP NAMESERVERS

カテゴリー：PPP / 一般コマンド

`SHOW PPP NAMESERVERS`

PPPのグローバル設定パラメーターである、DNSサーバーとWINSサーバー（IPCPで相手に教えるアドレス）の設定値を表示する。

入力・出力・画面例

    Manager > show ppp nameservers

      Name Server                      Address
      ------------------------------------------------
      Primary DNS .................... 172.20.28.1
      Secondary DNS .................. 172.20.22.10
      Primary WinS ................... 172.20.28.5
      Secondary WinS ................. Not Set
      ------------------------------------------------

表 1
Primary DNS Address | プライマリーDNSサーバーのIPアドレス
Secondary DNS Address | セカンダリーDNSサーバーのIPアドレス
Primary WinS Address | プライマリーWINSサーバーのIPアドレス
Secondary WinS Address | セカンダリーWINSサーバーのIPアドレス

関連コマンド

SET PPP DNSPRIMARY
SHOW PPP

参考

RFC1331, The Point-to-Point Protocol (PPP) for the Transmission of Multi-protocol Datagrams over Point-to-Point Links
RFC1332, The PPP Internet Protocol Control Protocol (IPCP)
RFC1333, PPP Link Quality Monitoring
RFC1334, PPP Authentication Protocols
RFC1548, The Point-to-Point Protocol (PPP)
RFC1549, PPP in HDLC Framing
RFC1570, PPP LCP Extensions
RFC1638, PPP Bridging Control Protocol (BCP)
RFC1661, The Point-to-Point Protocol (PPP)
RFC1662, PPP in HDLC-like Framing
RFC1877, PPP Internet Protocol Control Protocol Extensions for Name Server Addresses
RFC2516, A Method for Transmitting PPP Over Ethernet (PPPoE)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H