[index] CentreCOM AR550S コマンドリファレンス 2.9

# SET SNMP TARGETADDR

カテゴリー：運用・管理 / SNMP

`SET SNMP TARGETADDR=target [PARAMS=params] [IP=ipadd] [UDP=port]`

target: SNMPターゲット名（1〜32文字。大文字小文字を区別する）
params: SNMPターゲットパラメーターセット名（1〜32文字。大文字小文字を区別する）
ipadd: IPアドレス
port: UDPポート番号（1〜255）

（SNMPv3）ターゲット（通知メッセージの送信先）の設定を変更する。

パラメーター

TARGETADDR: SNMPターゲット名

PARAMS: SNMPターゲットパラメーターセット名。ADD SNMP TARGETPARAMSコマンドで定義したパラメーターセットの名前を指定する。

IP: ターゲットのIPアドレス

UDP: ターゲットのリスニングUDPポート。1〜255の範囲で指定する。省略時は162

関連コマンド

ADD SNMP TARGETADDR
ADD SNMP TARGETPARAMS
DELETE SNMP TARGETADDR
SHOW SNMP TARGETADDR
SHOW SNMP TARGETPARAMS

参考

RFC1155, Structure and Identification of Management Information for TCP/IP-based Internets
RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1239, Reassignment of Experimental MIBs to Standard MIBs
RFC1398, Definitions of Managed Objects for the Ethernet-like Interface Types
RFC1493, Definitions of Managed Objects for Bridges
RFC1514, Host Resources MIB
RFC1573, Evolution of the Interfaces Group of MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC2233, The Interfaces Group MIB using SMIv2
RFC2576, Coexistence between Version 1, Version 2, and Version 3 of the Internet-standard Network Management Framework
RFC2578, Structure of Management Information Version 2 (SMIv2)
RFC2579, Textual Conventions for SMIv2
RFC2580, Conformance Statements for SMIv2
RFC3410, Introduction and Applicability Statements for Internet Standard Management Framework
RFC3411, An Architecture for Describing Simple Network Management Protocol (SNMP) Management Frameworks
RFC3412, Message Processing and Dispatching for the Simple Network Management Protocol (SNMP)
RFC3413, Simple Network Management Protocol (SNMP) Applications
RFC3414, User-based Security Model (USM) for version 3 of the Simple Network Management Protocol (SNMPv3)
RFC3415, View-based Access Control Model (VACM) for the Simple Network Management Protocol (SNMP)
RFC3416, Version 2 of the Protocol Operations for the Simple Network Management Protocol (SNMP)
RFC3417, Transport Mappings for the Simple Network Management Protocol (SNMP)
RFC3418, Management Information Base (MIB) for the Simple Network Management Protocol (SNMP)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H