[index] CentreCOM AR550S コマンドリファレンス 2.9

# ENABLE SNMP COMMUNITY

カテゴリー：運用・管理 / SNMP

`ENABLE SNMP COMMUNITY=community`

community: SNMPコミュニティー名（1〜15文字。大文字小文字を区別する）

（SNMPv1/v2c）無効状態のSNMPコミュニティーを有効にする。

パラメーター

COMMUNITY: SNMPコミュニティー名

関連コマンド

DISABLE SNMP
DISABLE SNMP COMMUNITY
ENABLE SNMP
SHOW SNMP
SHOW SNMP COMMUNITY

参考

RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)

(C) 2005-2012 アライドテレシスホールディングス株式会社

PN: J613-M0710-03 Rev.H