[index] CentreCOM 8624PS コマンドリファレンス 2.8

# SHOW POE

カテゴリー：PoE / 一般コマンド

`SHOW POE [PORT={port-list|ALL}]`

port-list: スイッチポート番号（1〜。ハイフン、カンマを使った複数指定も可能）

PoE給電機能の一般情報、および、各ポートのPoE関連情報を表示する。

パラメーター

PORT: ポート番号。複数指定が可能。ALLを指定した場合はすべてのポートが対象となる（ただし、拡張スロットに拡張モジュールを装着しているときは、ALLを指定するとエラーになるので注意）。本パラメーターを指定した場合は、指定したポートのPoE関連情報が表示される。本パラメーターを省略した場合は、PoE給電機能の一般情報と各ポートのPoE関連情報が簡潔に一覧表示される。

入力・出力・画面例

    Manager > show poe

    PoE Global Power Status:

    Max Available Power .... 220 W
    Power Threshold ........ 95 percent
    Consumed Power ......... 11 W
    Available Power ........ 209 W
    Power Usage ............ 5.0 percent
    PowerDetect Mode ....... IEEE
    Min Shutdown Voltage ... 44.0 V
    Max Shutdown Voltage ... 57.0 V

    PoE All Ports Power Status Summary:

    Port  PoE Status  Consumed Power(mW)  Power State
    -------------------------------------------------------------------------------
    1     ENABLED           1900          ON  - Valid PD detected
    2     ENABLED              0          OFF - Detection in process
    3     ENABLED           1900          ON  - Valid PD detected
    4     ENABLED              0          OFF - Detection in process
    5     ENABLED           1900          ON  - Valid PD detected
    6     ENABLED              0          OFF - Detection in process
    7     ENABLED           6100          ON  - Valid PD detected
    8     ENABLED              0          OFF - Detection in process
    9     ENABLED              0          OFF - Detection in process
    10    ENABLED              0          OFF - Detection in process
    11    ENABLED              0          OFF - Detection in process
    12    ENABLED              0          OFF - Detection in process
    13    ENABLED              0          OFF - Detection in process
    14    ENABLED              0          OFF - Detection in process
    15    ENABLED              0          OFF - Detection in process
    16    ENABLED              0          OFF - Detection in process
    17    ENABLED              0          OFF - Detection in process
    18    ENABLED              0          OFF - Detection in process
    19    ENABLED              0          OFF - Detection in process
    20    ENABLED              0          OFF - Detection in process
    21    ENABLED              0          OFF - Detection in process
    22    ENABLED              0          OFF - Detection in process
    23    ENABLED              0          OFF - Detection in process
    24    ENABLED              0          OFF - Detection in process

    Manager > show poe port=3

    PoE Status of Port 3:
    -------------------------------------------------------------------------------
    PoE Status ......... ENABLED
    Power Limit ........ 15400 mW
    Power Priority ..... LOW
    Power State ........ ON  - Valid PD detected
    Power Consumed ..... 1900 mW
    Power Class ........ 1
    Voltage ............ 48.0 V
    Current ............ 40 mA

表 1：ポート無指定時
Max Available Power | 装置全体の供給可能電力量（W）
Power Threshold | PoE給電機能のログ出力/トラップ送信のしきい値（%）
Consumed Power | （受電機器による）現行の消費電力（W）
Available Power | （受電機器に割り当て可能な）現行の余剰電力（W）
Power Usage | 供給可能電力に対する消費電力の割合（%）
Power Detect Mode | 受電機器（PD）の検出方式。IEEEかLEGACY
Min Shutdown Voltage | 給電電圧の下限しきい値（V）。なんらかの原因で供給電圧がこの値を下回った場合、本製品は全ポートのPoE給電機能を無効化する。この値は固定値で変更不可
Max Shutdown Voltage | 給電電圧の上限しきい値（V）。なんらかの原因で供給電圧がこの値を上回った場合、本製品は全ポートのPoE給電機能を無効化する。この値は固定値で変更不可
PoE All Ports Power Status Summaryセクション | 各ポートのPoE関連情報が簡潔に表示される
Port | ポート番号
PoE Status | PoE給電機能の有効・無効
Consumed Power(mW) | ポートに接続されている受電機器の現行消費電力（mW）
Power State | ポートが給電中かどうか。ON（給電中）かOFF（停電中）。ON/OFFの後には簡単なステータスも表示される

表 2：ポート指定時
PoE Status | PoE給電機能の有効・無効
Power Limit | ポートの供給電力上限値（mW）
Power Priority | ポートの給電優先度。CRITICAL（最高）、HIGH（高）、LOW（低）のいずれか
Power State | ポートが給電中かどうか。ON（給電中）かOFF（停電中）。ON/OFFの後には簡単なステータスも表示される
Power Consumed | ポートに接続されている受電機器の現行消費電力（mW）
Power Class | ポートに接続されている受電機器の電力クラス。この情報は表示のみで、給電制御には使用されない
Voltage | ポートの供給電圧（V）
Current | ポートの供給電流（mA）

関連コマンド

DISABLE POE PORT
ENABLE POE PORT
SET POE DETECT
SET POE THRESHOLD

(C) 2005 - 2006 アライドテレシスホールディングス株式会社

PN: J613-M0785-02 Rev.B