[index] CentreCOM 8700SLシリーズ コマンドリファレンス 2.9

# DELETE IP ASPATHLIST

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-08 が必要

`DELETE IP ASPATHLIST=1..99 [ENTRY=1..4294967295]`

ASパスリストからエントリーを削除する。

パラメーター

ASPATHLIST: ASパスリスト番号

ENTRY: リスト内におけるエントリーの位置。省略時はすべてのエントリーが対象となる。

例

``■ ASパスリスト「1」からエントリー「3」を削除する。
`DELETE IP ASPATHLIST=1 ENTRY=3
` ■ ASパスリスト「2」の全エントリーを削除する。
`DELETE IP ASPATHLIST=2`

関連コマンド

ADD IP ASPATHLIST
SHOW IP ASPATHLIST

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2003 - 2010 アライドテレシスホールディングス株式会社

PN: J613-M0019-01 Rev.P