[index] CentreCOM 8948XL コマンドリファレンス 2.9

# DELETE IP PREFIXLIST

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-09 が必要

`DELETE IP PREFIXLIST=plist [ENTRY=1..65535]`

plist: プレフィックスリスト名（0〜15文字。英数字とアンダースコアを使用可能。大文字小文字を区別する）

プレフィックスリストからエントリーを削除する。

パラメーター

PREFIXLIST: プレフィックスリスト名

ENTRY: リスト内におけるエントリーの位置。省略時はすべてのエントリーが対象となる。

関連コマンド

ADD BGP PEER
ADD IP PREFIXLIST
ADD IP ROUTEMAP
SET BGP PEER
SET IP PREFIXLIST
SHOW IP PREFIXLIST

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L