[index] CentreCOM 8948XL コマンドリファレンス 2.9

# SHOW SNMP VIEW

カテゴリー：運用・管理 / SNMP

`SHOW SNMP VIEW[=view]`

view: SNMPビュー名（1〜32文字。大文字小文字を区別する）

（SNMPv3）ビューの設定内容を表示する。

パラメーター

VIEW: SNMPビュー名。ビュー名を指定しなかった場合は、定義されているビュー名の一覧が表示される。ビュー名を指定した場合は、指定したビューの設定内容が表示される。

入力・出力・画面例

    Manager > show snmp view

    SNMP View information:
      SNMP View name(s):
        most
        standard
        mib2notcpudp

    Manager > show snmp view=mib2notcpudp

    SNMP View information:
      View Name ....................... mib2notcpudp
        OID ........................... 1.3.6.1.2.1
          MIB ......................... mib-2
          Type ........................ include
          Row Status .................. active
        OID ........................... 1.3.6.1.2.1.6
          MIB ......................... tcp
          Type ........................ exclude
          Row Status .................. active
        OID ........................... 1.3.6.1.2.1.7
          MIB ......................... udp
          Type ........................ exclude
          Row Status .................. active

表 1
View Name | ビュー名
OID | ビューに含まれる（Type=include）または含まれない（Type=exclude）MIBノードのOID（Object Identifier）
MIB | OIDで示されるMIBノードの名前。OIDに該当するノード名がシステムに定義されている場合のみ表示される
Type | OIDで示されるMIBノードがビューに含まれているかどうか。includeなら含まれ、excludeなら含まれない
Row Status | ビューの状態。active、not in service、not readyのいずれか

備考・注意事項

ビュー内のエントリーはOIDの辞書順にソートされて表示される。

関連コマンド

ADD SNMP VIEW
DELETE SNMP VIEW

参考

RFC1155, Structure and Identification of Management Information for TCP/IP-based Internets
RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1239, Reassignment of Experimental MIBs to Standard MIBs
RFC1398, Definitions of Managed Objects for the Ethernet-like Interface Types
RFC1493, Definitions of Managed Objects for Bridges
RFC1514, Host Resources MIB
RFC1573, Evolution of the Interfaces Group of MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC2233, The Interfaces Group MIB using SMIv2
RFC2576, Coexistence between Version 1, Version 2, and Version 3 of the Internet-standard Network Management Framework
RFC2578, Structure of Management Information Version 2 (SMIv2)
RFC2579, Textual Conventions for SMIv2
RFC2580, Conformance Statements for SMIv2
RFC3410, Introduction and Applicability Statements for Internet Standard Management Framework
RFC3411, An Architecture for Describing Simple Network Management Protocol (SNMP) Management Frameworks
RFC3412, Message Processing and Dispatching for the Simple Network Management Protocol (SNMP)
RFC3413, Simple Network Management Protocol (SNMP) Applications
RFC3414, User-based Security Model (USM) for version 3 of the Simple Network Management Protocol (SNMPv3)
RFC3415, View-based Access Control Model (VACM) for the Simple Network Management Protocol (SNMP)
RFC3416, Version 2 of the Protocol Operations for the Simple Network Management Protocol (SNMP)
RFC3417, Transport Mappings for the Simple Network Management Protocol (SNMP)
RFC3418, Management Information Base (MIB) for the Simple Network Management Protocol (SNMP)

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L