[index] CentreCOM 8948XL コマンドリファレンス 2.9

# ADD SNMP COMMUNITY

カテゴリー：運用・管理 / SNMP

`ADD SNMP COMMUNITY=community [MANAGER=ipadd[/masklen]] [TRAPHOST=ipadd] [V1TRAPHOST=ipadd] [V2CTRAPHOST=ipadd]`

community: SNMPコミュニティー名（1〜15文字。大文字小文字を区別する）
ipadd: IPアドレス
masklen: マスク長（0〜32）

（SNMPv1/v2c）SNMPコミュニティーに管理ステーション、トラップホストを追加する。

パラメーター

COMMUNITY: SNMPコミュニティー名

MANAGER: SNMPオペレーションを許可する管理ステーション。マスク長を付加することで範囲指定も可能。本エージェントは、MANAGERに登録されていないホストからのSNMP要求には応答しない。ただし、SNMPコミュニティーのOPENパラメーターがYESの場合は、MANAGERパラメーターの設定にかかわらず、すべてのSNMP要求に応答する。

TRAPHOST: SNMPv1トラップの送信先ホスト。ここで指定したホストにはSNMPv1形式のトラップが送信される。

V1TRAPHOST: SNMPv1トラップの送信先ホスト。TRAPHOSTパラメーターと同じ。

V2CTRAPHOST: SNMPv2cトラップの送信先ホスト。ここで指定したホストにはSNMPv2c形式のトラップが送信される。

例

``■ SNMPコミュニティー「public」に管理ステーションを追加する。
`ADD SNMP COMMUNITY=public MANAGER=192.168.20.5`

備考・注意事項

SNMPトラップは、ENABLE SNMP COMMUNITY TRAPコマンドを実行してコミュニティーのトラップ設定を有効にしないと送信されないので注意が必要。
TRAPHOST（またはV1TRAPHOST）とV2CTRAPHOSTに同じホストを指定してもよい

関連コマンド

CREATE SNMP COMMUNITY
DELETE SNMP COMMUNITY
DESTROY SNMP COMMUNITY
DISABLE SNMP COMMUNITY
DISABLE SNMP COMMUNITY TRAP
ENABLE SNMP COMMUNITY
ENABLE SNMP COMMUNITY TRAP
SET SNMP COMMUNITY
SHOW SNMP COMMUNITY

参考

RFC1155, Structure and Identification of Management Information for TCP/IP-based Internets
RFC1157, A Simple Network Management Protocol (SNMP)
RFC1213, Management Information Base for Network Management of TCP/IP-based internets: MIB-II
RFC1239, Reassignment of Experimental MIBs to Standard MIBs
RFC1398, Definitions of Managed Objects for the Ethernet-like Interface Types
RFC1493, Definitions of Managed Objects for Bridges
RFC1514, Host Resources MIB
RFC1573, Evolution of the Interfaces Group of MIB-II
RFC1901, Introduction to Community-based SNMPv2
RFC1902, Structure of Management Information for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1903, Textual Conventions for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1904, Conformance Statements for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1905, Protocol Operations for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1906, Transport Mappings for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC1907, Management Information Base for Version 2 of the Simple Network Management Protocol (SNMPv2)
RFC2233, The Interfaces Group MIB using SMIv2

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L