[index] CentreCOM 8948XL コマンドリファレンス 2.9

# DELETE IP ROUTEMAP

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-09 が必要

`DELETE IP ROUTEMAP=routemap [ENTRY=1..4294967295]
DELETE IP ROUTEMAP=routemap ENTRY=1..4294967295 MATCH={ASPATH|COMMUNITY|NEXTHOP|ORIGIN|PREFIXLIST|TAG}
DELETE IP ROUTEMAP=routemap ENTRY=1..4294967295 SET={ASPATH|BGPDAMPID|COMMUNITY|LOCALPREF|MED|ORIGIN}`

routemap: ルートマップ名（0〜15文字。英数字とアンダースコアを使用可能。大文字小文字を区別する）

ルートマップからエントリーを削除する。または、ルートマップのエントリーからMATCH節あるいはSET節を削除する。
使用中のルートマップは削除できない。

パラメーター

ROUTEMAP: ルートマップ名

ENTRY: ルートマップ内のエントリー番号。省略時はすべてのエントリーが削除対象となる。MATCH節、SET節を削除するときは、必ずエントリー番号を指定しなくてはならない。

MATCH: 指定したエントリーから削除するMATCH節の種類

SET: 指定したエントリーから削除するSET節の種類

例

``■ ルートマップ「outi」のエントリー「2」からLOCAL_PREF属性をセットするSET節を削除する。
`DELETE IP ROUTEMAP=outi ENTRY=2 SET=LOCALPREF`

関連コマンド

ADD IP ROUTEMAP
SET IP ROUTEMAP
SHOW IP ROUTEMAP

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L