[index] CentreCOM 8948XL コマンドリファレンス 2.9

# DELETE IP COMMUNITYLIST

カテゴリー：IP / 経路制御（BGP-4）
備考：フィーチャーライセンス AT-FL-09 が必要

`DELETE IP COMMUNITYLIST=1..99 [ENTRY=1..4294967295]`

コミュニティーリストからエントリーを削除する。

パラメーター

COMMUNITYLIST: コミュニティーリスト番号

ENTRY: リスト内におけるエントリーの位置。省略時はすべてのエントリーが対象となる。

例

``■ コミュニティーリスト「1」からエントリー「3」を削除する。
`DELETE IP COMMUNITYLIST=1 ENTRY=3
` ■ コミュニティーリスト「2」の全エントリーを削除する。
`DELETE IP COMMUNITYLIST=2`

関連コマンド

ADD IP COMMUNITYLIST
SHOW IP COMMUNITYLIST

参考

RFC1771, A Border Gateway Protocol 4 (BGP-4)
RFC1772, Application of the Border Gateway Protocol in the Internet
RFC1930, Guidelines for creation, selection, and registration of an Autonomous System (AS)
RFC1997, BGP Communities Attribute
RFC2385, Protection of BGP Sessions via the TCP MD5 Signature Option
RFC2439, BGP Route Flap Damping
RFC2796, BGP Route Reflection - An Alternative to Full Mesh IBGP
RFC2842, Capabilities Advertisement with BGP-4
RFC2918, Route Refresh Capability for BGP-4
RFC3065, Autonomous System Confederations for BGP

(C) 2004 - 2008 アライドテレシスホールディングス株式会社

PN: J613-M0021-12 Rev.L