# show counter mrp

モード
  特権EXECモード
カテゴリー
  L2スイッチング / MRP

## 構文

コマンド構文

`# show counter mrp [global | ring <1-65535>]`

## コマンド説明

MRPリングの統計カウンターを表示する。

## パラメーター

`global`
  グローバルMRPカウンターのみを無効にする
`ring <1-65535>`
  MRPリングIDのカウンターのみを表示する

## 使用例

    awplus# show counter mrp
    Media Redundancy Protocol Global Counters

    MRP Started             ....... 2
    MRP Dispatcher          ....... 19102219
    MRP Timer Tick          ....... 17373917
    MRP Packet RX           ....... 1728302
    MRP Packet RX Error     ....... 0
    MRP Packet TX           ....... 1728303
    MRP Packet TX Error     ....... 0

    Media Redundancy Protocol Ring 1 Counters

    Port 1 PDUs Received
    MRP_Test              ......... 864150
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 1 PDUs Transferred
    MRP_Test              ......... 864152
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 2 PDUs Received
    MRP_Test              ......... 864152
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 2 PDUs Transferred
    MRP_Test              ......... 864152
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Other Counters
    State Changes         ......... 6
    Port Blocked Set      ......... 4
    Port Forwarding Set   ......... 2

    awplus# show counter mrp global
    Media Redundancy Protocol Global Counters

    MRP Started             ....... 2
    MRP Dispatcher          ....... 19211403
    MRP Timer Tick          ....... 17473175
    MRP Packet RX           ....... 1738228
    MRP Packet RX Error     ....... 0
    MRP Packet TX           ....... 1738229
    MRP Packet TX Error     ....... 0

    awplus# show counter mrp ring 1
    Media Redundancy Protocol Ring 1 Counters

    Port 1 PDUs Received
    MRP_Test              ......... 871675
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 1 PDUs Transferred
    MRP_Test              ......... 871677
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 2 PDUs Received
    MRP_Test              ......... 871677
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Port 2 PDUs Transferred
    MRP_Test              ......... 871677
    MRP_TopologyChange    ......... 0
    MRP_LinkUp            ......... 0
    MRP_LinkDown          ......... 0

    Other Counters
    State Changes         ......... 6
    Port Blocked Set      ......... 4
    Port Forwarding Set   ......... 2

## 関連コマンド